**Instructions for attaching Magnetic control device and Tensioner on glass**

 Stick the Tensioner on the glass without any preload of the internal spring!!